**Highest Priority (Red - Must Have)**

1. **Hard Hats**: Must be worn at all times on site. (Tags: “construction,” “general safety”) **[Must Have]**
2. **LOTO Procedures**: Lockout/tagout for live circuits to prevent accidental energization. (Tags: “electrical,” “live circuits”) **[Must Have]**
3. **Harness Use**: Required for workers at elevated locations to prevent falls. (Tags: “working at heights”) **[Must Have]**
4. **Guardrails and Nets**: Must be installed in areas where falls are a risk. (Tags: “working at heights,” “guardrails”) **[Must Have]**
5. **Anchorage Points**: Secure anchorage points must be available for fall arrest equipment. (Tags: “fall arrest,” “working at heights”) **[Must Have]**
6. **Respiratory Protection**: Must be used if exposed to dust, fumes, or toxic substances. (Tags: “dust,” “fumes,” “chemical handling”) **[Must Have]**
7. **Emergency Exits**: Must be clearly marked and unobstructed at all times. (Tags: “emergency,” “general safety”) **[Must Have]**

**Moderate Priority (Amber - Mandatory)**

1. **Eye Protection**: Safety goggles or face shields mandatory when needed, especially near machinery or chemicals. (Tags: “machinery,” “chemical handling”) **[Mandatory]**
2. **Ear Protection**: Required in high-noise areas to prevent hearing damage. (Tags: “high noise,” “construction”) **[Mandatory]**
3. **Non-Slip Footwear**: Mandatory for all workers to reduce slip hazards. (Tags: “general safety”) **[Mandatory]**
4. **Gloves for Electrical Work**: Specific gloves mandatory for electrical tasks to prevent shocks. (Tags: “electrical,” “live circuits”) **[Mandatory]**
5. **High-Voltage Signage**: Clear signage mandatory around high-voltage equipment to alert personnel. (Tags: “electrical,” “high voltage”) **[Mandatory]**
6. **Restricted Area Signage**: Mandatory in hazardous zones to control access. (Tags: “hazardous areas,” “restricted zones”) **[Mandatory]**
7. **Flammable Material Precautions**: No open flames allowed near flammable materials. (Tags: “flammable materials”) **[Mandatory]**
8. **Hazardous Substance Labeling**: Mandatory proper labeling and storage for all hazardous substances. (Tags: “hazardous materials”) **[Mandatory]**

**Lower Priority (Green - Okay to Have)**

1. **Scaffold Training**: Workers should be trained in safe scaffold practices. (Tags: “scaffolding,” “training”) **[Okay to Have]**
2. **Access to Scaffolds**: Ladders or stairs should be provided for scaffold access. (Tags: “scaffolding,” “access”) **[Okay to Have]**
3. **High-Visibility Vests**: Should be worn for enhanced visibility. (Tags: “construction,” “general safety”) **[Okay to Have]**
4. **Cord Protection**: Cords should be kept clear of walkways and undamaged. (Tags: “electrical,” “general safety”) **[Okay to Have]**
5. **Waste Disposal**: Hazardous and non-hazardous materials should be disposed of correctly. (Tags: “waste,” “hazardous materials”) **[Okay to Have]**
6. **Use of Slings, Chains, and Ropes**: Recommended for safe handling of heavy materials. (Tags: “material lifting,” “cranes,” “rigging”) **[Okay to Have]**
7. **Proper Lifting Techniques**: Workers should use safe lifting techniques. (Tags: “manual handling,” “lifting”) **[Okay to Have]**
8. **Vibration-Reducing Gloves/Tools**: Recommended for high-vibration tasks to reduce strain. (Tags: “vibration,” “tools”) **[Okay to Have]**
9. **Workstation Adjustments**: Adjustments should be made for ergonomic comfort where applicable. (Tags: “ergonomics,” “comfort”) **[Okay to Have]**