### Highest Priority (Red - Non Negotiable)

1. **Hard Hats**: Must be worn at all times on site.  
   **Tags:** “construction,” “general safety,” **“scaffolding”** [Non Negotiable]
2. **LOTO Procedures**: Lockout/tagout for live circuits to prevent accidental energization.  
   **Tags:** “electrical,” “live circuits” [Non Negotiable]
3. **Harness Use**: Required for workers at elevated locations to prevent falls.  
   **Tags:** “working at heights,” **“scaffolding,” “heavy machinery”** [Non Negotiable]
4. **Guardrails and Nets**: Must be installed in areas where falls are a risk.  
   **Tags:** “working at heights,” “guardrails,” **“scaffolding,” “construction”** [Non Negotiable]
5. **Anchorage Points**: Secure anchorage points must be available for fall arrest equipment.  
   **Tags:** “fall arrest,” “working at heights,” **“heavy machinery,” “scaffolding”** [Non Negotiable]
6. **Respiratory Protection**: Must be used if exposed to dust, fumes, or toxic substances.  
   **Tags:** “dust,” “fumes,” “chemical handling,” “construction” [Non Negotiable]
7. **Emergency Exits**: Must be clearly marked and unobstructed at all times.  
   **Tags:** “emergency,” “general safety,” “construction” [Non Negotiable]

### Moderate Priority (Amber - Strongly Advised)

1. **Eye Protection**: Safety goggles or face shields strongly advised near machinery or chemicals.  
   **Tags:** “machinery,” “chemical handling,” **“heavy machinery”** [Strongly Advised]
2. **Ear Protection**: Required in high-noise areas to prevent hearing damage.  
   **Tags:** “high noise,” “construction,” **“heavy machinery”** [Strongly Advised]
3. **Non-Slip Footwear**: Strongly advised for all workers to reduce slip hazards.  
   **Tags:** “general safety,” “construction” [Strongly Advised]
4. **Gloves for Electrical Work**: Specific gloves strongly advised for electrical tasks to prevent shocks.  
   **Tags:** “electrical,” “live circuits” [Strongly Advised]
5. **High-Voltage Signage**: Clear signage around high-voltage equipment to alert personnel.  
   **Tags:** “electrical,” “high voltage” [Strongly Advised]
6. **Restricted Area Signage**: Strongly advised in hazardous zones to control access.  
   **Tags:** “hazardous areas,” “restricted zones,” “construction” [Strongly Advised]
7. **Flammable Material Precautions**: No open flames allowed near flammable materials.  
   **Tags:** “flammable materials” [Strongly Advised]
8. **Hazardous Substance Labeling**: Proper labeling and storage for all hazardous substances.  
   **Tags:** “hazardous materials” [Strongly Advised]

### Lower Priority (Green - Advised)

1. **Scaffold Training**: Workers should be trained in safe scaffold practices.  
   **Tags:** “scaffolding,” “training,” “construction” [Advised]
2. **Access to Scaffolds**: Ladders or stairs should be provided for scaffold access.  
   **Tags:** “scaffolding,” “access,” “construction” [Advised]
3. **High-Visibility Vests**: Should be worn for enhanced visibility.  
   **Tags:** “construction,” “general safety” [Advised]
4. **Cord Protection**: Cords should be kept clear of walkways and undamaged.  
   **Tags:** “electrical,” “general safety,” “construction” [Advised]
5. **Waste Disposal**: Hazardous and non-hazardous materials should be disposed of correctly.  
   **Tags:** “waste,” “hazardous materials” [Advised]
6. **Use of Slings, Chains, and Ropes**: Recommended for safe handling of heavy materials.  
   **Tags:** “material lifting,” “cranes,” “rigging,” **“heavy machinery”** [Advised]
7. **Proper Lifting Techniques**: Workers should use safe lifting techniques.  
   **Tags:** “manual handling,” “lifting,” “construction” [Advised]
8. **Vibration-Reducing Gloves/Tools**: Recommended for high-vibration tasks to reduce strain.  
   **Tags:** “vibration,” “tools” [Advised]
9. **Workstation Adjustments**: Adjustments should be made for ergonomic comfort where applicable.  
   **Tags:** “ergonomics,” “comfort” [Advised]