**Hard Hats**: Worn at all times on site is mandatory

**Guardrails and Nets**: For areas where falls are a risk is mandatory

**Harness Use**: Required for workers only at elevated locations and is must

**Anchorage Points**: Secure points for fall arrest equipment.

**Cover or Mark Floor Openings**: To prevent falls is required

**LOTO Procedures**: Lockout/tagout for live circuits is must

**High-Voltage Signage**: Required around electrical equipment is must if visible.

**Emergency Exits**: Marked and unobstructed as long as it is clearly visible in the picture

**Respiratory Protection**: Use if exposed to dust, fumes, or toxic substances.

**Eye Protection**: Safety goggles or face shields when any work related to fire or similar is done.

**Ear Protection**: Required in high-noise areas only

**Non-Slip Footwear**: Essential for all workers and is mandatory

**Gloves for Chemical Handling**: Specific types based on tasks only.

**Restricted Area Signage**: Clear signs for hazardous zones as long as it is clearly visible

**Barricades and Warnings**: Around excavation sites.

**Flammable Material Precautions**: No open flames near flammable substances.

**Hazardous Substance Labeling**: Proper labeling and storage.

**Scaffold Training**: Workers must be trained in safe practices.

**Access to Scaffolds**: Provide ladders or stairs for scaffold access.

**High-Visibility Vests**: Required for visibility.

**Cord Protection**: Prevent damage and keep cords clear of walkways.

**Waste Disposal**: Proper handling of hazardous and non-hazardous materials.

**Use of Slings, Chains, and Ropes**: For lifting heavy materials safely.

**Proper Lifting Techniques**: Bend knees, keep back straight.

**Vibration-Reducing Gloves/Tools**: Use for high-vibration tasks.

**Workstation Adjustments**: For worker comfort where applicable.

**Gloves for Electrical Work**: Specific types based on tasks.

**Chemical Handling Gloves**: Specific gloves based on tasks.

**Scaffold Training**: Workers must be trained in safe practices.